# Form OP-UA2 - Instructions

# Stationary Reciprocating Internal Combustion Engine Attributes

# Texas Commission on Environmental Quality

**General:**

This form is used to provide a description and data pertaining to all stationary reciprocating internal combustion (SRIC) engines with potentially applicable requirements associated with a particular regulated entity number and application. Each table number, along with the possibility of a corresponding letter (i.e., Table 1a, Table 1b), corresponds to a certain state or federal rule. If the rule on the table is not potentially applicable to an SRIC engine, then it should be left blank and need not be submitted with the application. If the codes entered by the applicant show negative applicability to the rule or sections of the rule represented on the table, then the applicant need not complete the remainder of the table(s) that corresponds to the rule. Further instruction as to which questions should be answered and which questions should not be answered are located in the “Specific” section of the instruction text. The following is included in this form:

2BTitle 30 Texas Administrative Code Chapter 117 (30 TAC Chapter 117), Subchapter B: Combustion Control at Major Industrial, Commercial, and Institutional Sources in Ozone Nonattainment Areas

[**Table 1a - 1c**](#Table_1a)**: Title 30 Texas Administrative Code Chapter 117 (30 TAC Chapter 117), Subchapter B: Combustion Control at Major Industrial, Commercial, and Institutional Sources in Ozone Nonattainment Areas**

[**Table 2a - 2c**](#Table_2a)**: 3B**[**44T**](#Table_2a)**44TTitle 40 Code of Federal Regulations Part 63 (40 CFR Part 63), Subpart ZZZZ: National Emission Standards for Hazardous Air Pollutants for Stationary Reciprocating Internal Combustion Engines.**

[**Table 3**](#Table_3)**: Title 30 Texas Administrative Code Chapter 117 (30 TAC Chapter 117), Subchapter E: Multi-Region Combustion Control, Division 4: East Texas Combustion**

[**Table 4a - 4b**](#Table_4a)**: Title 40 Code of Federal Regulations Part 60 (40 CFR Part 60), Subpart JJJJ: Standards of Performance for Stationary Spark Ignition Internal Combustion Engines**

[**Table 5a - 5c**](#Table_5a)**: Title 40 Code of Federal Regulations Part 60 (40 CFR Part 60), Subpart IIII: Standards of Performance for Stationary Compression Ignition Internal Combustion Engines**

The application area name from Form OP-1 (Site Information Summary) must appear in the header of each page for the purpose of identification for the initial submittal. The date of the initial form submittal must also be included and should be consistent throughout the application (MM/DD/YYYY). Leave the permit number blank for the initial form submittal. If this form is included as part of the permit revision process, enter the permit number assigned by the TCEQ, the area name (from Form OP-1), the date of the revision submittal.

Unit attribute questions that do not require a response from all applicants are preceded by qualification criteria in the instructions. If the unit does not meet the qualification criteria, a response to the question is not required. Anytime a response is not required based on the qualification criteria, leave the space on the form blank.

Notwithstanding any qualification criteria in the form instructions or information provided in other TCEQ guidance, the applicant may leave an attribute question blank (or indicate “N/A” for “Not Applicable”) if the attribute is not needed for the applicable requirement determinations of a regulation for a unit.

Please note that for general operating permit (GOP) applications, responses may be required for questions on this form which are not included as a column in the applicable GOP table. These responses may be needed to determine applicability of certain requirements within a single row of the GOP permit table.

In some situations, the applicant has the option of selecting alternate requirements, limitations, and/or practices for a unit. Note that these alternate requirements, limitations, and/or practices must have the required approval from the TCEQ

Executive Director and/or the U.S. Environmental Protection Agency Administrator before the federal operating permit application is submitted.

The Texas Commission on Environmental Quality (TCEQ) requires that a Core Data Form be submitted on all incoming registrations unless all of the following are met: the Regulated Entity and Customer Reference numbers have been issued by the TCEQ and no core data information has changed. The Central Registry, a common record area of the TCEQ, maintains information about TCEQ customers and regulated activities, such as company names, addresses, and telephone numbers. This information is commonly referred to as “core data.” The Central Registry provides the regulated community with a central access point within the agency to check core data and make changes when necessary. When core data about a facility is moved to the Central Registry, two new identification numbers are assigned: the Customer Reference (CN) number and the Regulated Entity (RN) number. The Core Data Form is required if facility records are not yet part of the Central Registry or if core data for a facility has changed. If this is the initial registration, permit, or license for a facility site, then the Core Data Form must be completed and submitted with application or registration forms. If amending, modifying, or otherwise updating an existing record for a facility site, the Core Data Form is not required, unless any core data information has changed. To review additional information regarding the Central Registry, go to the TCEQ website at [44Twww.tceq.texas.gov/permitting/central\_registry/index.html44T](https://www.tceq.texas.gov/permitting/central_registry/index.html).

**Specific:**

**[Table 1a](#Tbl_1a): Title 30 Texas Administrative Code Chapter 117 (30 TAC Chapter 117), Subchapter B: Combustion Control at Major Industrial, Commercial, and Institutional Sources in Ozone Nonattainment Areas**

* Complete this table for SRIC engines that meet the following criteria:
* located at a site that is a major source of NOx, as defined in 30 TAC Chapter 117: and,
* located in the Houston/Galveston/Brazoria, Beaumont/Port Arthur, or Dallas/Fort Worth Eight-Hour Ozone Nonattainment Areas; and
* located at a site that is not an electric power generating system owned or operated by an electric cooperative, municipality, river authority, public utility or a Public Utility Commission of Texas regulated utility; or,
* if located in Parker County, the site does not generate electric power for compensation

Unit ID No.:

Enter the identification number (ID No.) for the SRIC engines (maximum 10 characters) as listed on Form OP-SUM (Individual Unit Summary).

SOP/GOP Index No.:

Site operating permit (SOP) applicants should indicate the SOP index number for the unit or group of units (maximum 15 characters consisting of numeric, alphanumeric characters, and/or dashes prefixed by a code for the applicable regulation [i.e., 60KB-XXXX]). GOP applicants should indicate the appropriate GOP index number in this column from the applicable GOP table (SSS-FF-XXX). Applicants should complete all applicable GOP attribute information before determining the GOP index number. For additional information relating to SOP index numbers, please go to the TCEQ website at [www.tceq.texas.gov/permitting/air/guidance/titlev/tv\_fop\_guidance.html](https://www.tceq.texas.gov/permitting/air/guidance/titlev/tv_fop_guidance.html).

* Complete “Horsepower Rating” if located in the Beaumont/Port Arthur or Dallas/Fort Worth Eight-Hour Ozone Nonattainment Areas.

Horsepower Rating:

Select one of the following options for the HP rating. Enter the code on the form.

For SRIC engines located in the Beaumont/Port Arthur Ozone Nonattainment Areas:

**Code Description**

300- HP is less than 300 (and unit is not a lean-burn gas-fired opt-in unit)

300+ HP is greater than or equal to 300

150+E2Y Lean-burn, gas-fired SRIC with HP greater than or equal to 150 that is exempt from RACT requirements under 30 TAC § 117.103(b) but is included under either a Source Cap or an Alternative Plant-Wide Emission Specification in 30 TAC §§ 117.123(a) or 117.115(a) as an opt‑in unit (for SOP applications only)

For SRIC engines located in the Dallas/Fort Worth Eight-Hour Ozone Nonattainment Area:

**Code Description**

50- HP is less than 50

50+ HP is greater or equal to than 50

* **Continue if application area is located in the Houston/Galveston/Brazoria or Dallas/Fort Worth Eight-Hour Ozone Nonattainment Areas; or if in the Beaumont/Port Arthur Ozone Nonattainment Areas and “Horsepower Rating” is “300+” or “150+E2Y”**
* Complete “RACT Date Placed in Service” if located in the Beaumont/Port Arthur Ozone Nonattainment Area and “Horsepower Rating” is “300+.” If “Horsepower Rating” is “150+E2Y,” go to “Fuel Fired” and provide information from that point forward.

RACT Date Placed in Service:

Select one of the following options for the date placed in service. Enter the code on the form.

**Code Description**

92- On or before November 15, 1992

92-93 After November 15, 1992 and on or before June 9, 1993

93-FCD After June 9, 1993 and before the final compliance date specified in 30 TAC § 117.9000

FCD+ After June 9, 1993 and on or after the final compliance date specified in 30 TAC § 117.9000

* Complete “Functionally Identical Replacement” only if “RACT Date Placed in Service” is “93-FCD.”

Functionally Identical Replacement:

Select one of the following options to identify if the unit is a functionally identical replacement for a unit or group of units that were in service on or before November 15, 1992. Enter the code on the form.

**Code Description**

YES Unit is a functionally identical replacement

NO Unit is not a functionally identical replacement

* **Do not continue if located in the Beaumont/Port Arthur Ozone Nonattainment Area and:**
* “Date Placed in Service” is “92-93” or “FCD+”; or
* “Date Placed in Service” is “93-FCD” and “Functionally Identical Replacement” is “NO.”

Type of Service:

Select one of the following options for the type of service. Enter the code on the form.

For SRIC engines located in the Beaumont/Port Arthur Ozone Nonattainment Areas:

**Code Description**

EXEMPT Used in research and testing, performance verification testing, solely to power other engines or turbines during startup, in response to and during the existence of any officially declared disaster or state of emergency or directly and exclusively in agricultural operations

EMERG Used exclusively in emergency situations [claiming the emergency service exemption under 30 TAC § 117.103(a)(6)(D)]

DIESEL Any stationary diesel engine

850- Demonstrated to operate less than 850 hours per year, based on a rolling 12-month average (low annual capacity factor) [claiming exemption 30 TAC § 117.103(b)(2)]

ENG Any other SRIC engine

For SRIC engines located in the Houston/Galveston/Brazoria Ozone Nonattainment Area:

**Code Description**

EXEMPT Used in research and testing, performance verification testing, solely to power other engines or turbines during startup, in response to and during the existence of any officially declared disaster or state of emergency or directly and exclusively in agricultural operations

EMERG Used exclusively in emergency situations [claiming the emergency service exemption under 30 TAC§ 117.303(a)(6)(D)] (exemption is not available for new, modified, reconstructed, or relocated diesel fuel fired SRIC engines placed into service on or after October 1, 2001)

D2001- Existing diesel fuel-fired engine placed into service before October 1, 2001, operated less than 100 hours/year, on a rolling 12-month average that has not been modified, reconstructed, or relocated on or after October 1, 2001 [claiming exemption 30 TAC § 117.303(a)(10)]

D2001+ New, modified, reconstructed or relocated diesel fuel-fired engine, placed into service on or after October 1, 2001, operated less than 100 hours/year, on a rolling 12-month average (other than emergency situations) that meets the corresponding emission standard for non-road engines listed in 40 CFR § 89.112(a), Table 1 (October 23, 1998) and in effect at the time of installation [claiming exemption 30 TAC § 117.303(a)(11)]

ENG Any other SRIC engine

For SRIC engines located in the Dallas/Fort Worth Eight-Hour Ozone Nonattainment Area:

**Code Description**

EXEMPT Used in research and testing, performance verification testing, solely to power other engines or turbines during startup, in response to and during the existence of any officially declared disaster or state of emergency or directly and exclusively in agricultural operations

EMERG Used exclusively in emergency situations [claiming the emergency service exemption under 30 TAC § 117.403(a)(7)(D)] (exemption is not available for new, modified, reconstructed, or relocated diesel fuel fired SRIC engines placed into service on or after June 1, 2007)

W-EMER Located in Wise County and used exclusively in emergency situations [claiming the emergency service exemption under 30 TAC § 117.403(b)(2)(D)]

D2007- Existing diesel fuel-fired engine placed into service before June 1, 2007, operated less than 100 hours/year, on a rolling 12-month average that has not been modified, reconstructed, or relocated on or after June 1, 2007 [claiming exemption 30 TAC § 117.403(a)(8)]

D2007+ Diesel fuel-fired engine, placed into service on or after June 1, 2007, operated less than 100 hours/year, on a rolling 12-month average (other than emergency situations) that meets the requirements for non-road engines [per 30 TAC § 117.403(a)(9)]

ENG Any other SRIC engine

* **Continue if “Type of Service” is “ENG,” “W-EMER,” or “EMERG.”**

Fuel Fired:

Select one of the following options for the fuel fired by the engine. Enter the code on the form.

For GOP applications:

**Code Description**

NG Natural Gas (Engines authorized to operate under GOPs 511, 512, 513 and 514 must select this option except for black start engines, fire pump engines, emergency engines, and engines operated less than 100 hours per year, as allowed by the rule)

LFG Landfill Gas

DIG Digester Gas

ORG Renewable, Non-fossil fuel gas other than landfill or digester gas

DSL Petroleum-based diesel fuel

B100 Pure or “neat” biodiesel fuel

BXX Blends of petroleum-based and biodiesel fuel

DUAL Dual-fuel where at least one of the fuels is a fossil fuel

DUALN Dual-fuel where both fuels are renewable non-fossil fuels

For SOP applications:

**Code Description**

NG Natural Gas

LFG Landfill Gas

ORG Renewable, Non-fossil fuel gas other than landfill gas

OFG Fuel gas other than natural gas, landfill gas, and renewable, non-fossil fuel gas (propane, butane, refinery fuel gas, etc.)

DSL Diesel fuel

B100 Pure or “neat” biodiesel fuel

BXX Blends of petroleum-based and biodiesel fuel

DUAL Dual-fuel where at least one of the fuels is a fossil fuel

DUALN Dual-fuel where both fuels are renewable non-fossil fuels

* **Do not continue if in Dallas/Fort Worth Eight-Hour Ozone Nonattainment Area and “Horsepower Rating” is “50-” and “Fuel Fired” is “NG,” “LFG,” “ORG” or “OFG.”**
* Continue only if “Type of Service” is “ENG;” or if “Horsepower Rating” is “150+E2Y.”

Engine Type:

Select one of the following options for the engine type as defined in 30 TAC Chapter 117. Enter the code on the form.

**Code Description**

LEANBURN Lean-burn

RICHBURN Rich-burn

* Complete “ESAD Date Placed in Service” only for the following:
* GOP or SOP applications for sites located in the Houston/Galveston/Brazoria Ozone Nonattainment Area and “Fuel Fired” is NOT “NG,” “LFG,” “ORG” or “OFG;” or
* GOP or SOP applications for sites located in the Dallas/Fort Worth Eight-Hour Ozone Nonattainment Area and “Fuel Fired” is NOT “DUAL” or “DUALN.”

ESAD Date Placed in Service:

Select one of the following options for the date the engine was placed into service. Enter the code on the form.

For dual fuel engines located in the Houston/Galveston/Brazoria Ozone Nonattainment Area.

**Code Description**

2001- Placed into service on or prior to December 31, 2000.

2001+ Placed into service after December 31, 2000.

For diesel engines located in the Houston/Galveston Ozone Nonattainment Area, please select the code that defines the most recent date that the engine was installed, modified, reconstructed, or relocated.

**Code Description**

-01 Placed into service before October 1, 2001 and has not been modified, reconstructed, or relocated on or after October 1, 2001.

01-02 Installed, modified, reconstructed, or relocated on or after October 1, 2001 but before October 1, 2002.

02-03 Installed, modified, reconstructed, or relocated on or after October 1, 2002 but before October 1, 2003.

03-04 Installed, modified, reconstructed, or relocated on or after October 1, 2003 but before October 1, 2004.

04-05 Installed, modified, reconstructed, or relocated on or after October 1, 2004 but before October 1, 2005.

05-06 Installed, modified, reconstructed, or relocated on or after October 1, 2005 but before October 1, 2006.

06-07 Installed, modified, reconstructed, or relocated on or after October 1, 2006 but before October 1, 2007.

07+ Installed, modified, reconstructed, or relocated on or after October 1, 2007.

For gas fired lean-burn engines located in the Dallas/Fort Worth Eight-Hour Ozone Nonattainment Area.

**Code Description**

2007- Placed into service prior to June 1, 2007, and not modified, reconstructed, or relocated on or after June 1, 2007

2007+ Placed into service, modified, reconstructed, or relocated on or after June 1, 2007

2015- Placed into service prior to June 1, 2015, and not modified, reconstructed, or relocated on or after June 1, 2015

2015+ Placed into service, modified, reconstructed, or relocated on or after June 1, 2015.

For diesel engines located in the Dallas/Fort Worth Eight-Hour Ozone Nonattainment Area, please select the code that defines the most recent date that the engine was installed, modified, reconstructed, or relocated.

**Code Description**

3109- Placed into service before March 1, 2009 and has not been modified, reconstructed, or relocated on or after March 1, 2009.

3109+ Installed, modified, reconstructed, or relocated on or after March 1, 2009.

* Complete “Diesel HP Rating” only for sites located in the Dallas/Fort Worth Eight-Hour or Houston/Galveston/Brazoria Ozone Nonattainment Area and “Fuel Fired” is “DSL,” “B100” or “BXX.”

Diesel HP Rating:

Select one of the following options for the horsepower rating of the diesel engine. Enter the code on the form.

For diesel SRIC engines located in the Houston/Galveston/Brazoria Ozone Nonattainment Area:

**Code Description**

11- Horsepower rating is less than 11 HP.

11-25 Horsepower rating is 11 HP or greater, but less than 25 HP.

25-50 Horsepower rating is 25 HP or greater, but less than 50 HP.

50-100 Horsepower rating is 50 HP or greater, but less than 100 HP.

100-175 Horsepower rating is 100 HP or greater, but less than 175 HP.

175-300 Horsepower rating is 175 HP or greater, but less than 300 HP.

300-600 Horsepower rating is 300 HP or greater, but less than 600 HP.

600-750 Horsepower rating is 600 HP or greater, but less than 750 HP.

750+ Horsepower rating is 750 HP or greater.

For diesel SRIC engines located in the Dallas/Fort Worth Eight-Hour Ozone Nonattainment Area:

**Code Description**

50- Horsepower rating is less than 50 HP.

50-100 Horsepower rating is 50 HP or greater, but less than 100 HP.

100-750 Horsepower rating is 100 HP or greater, but less than 750 HP.

750+ Horsepower rating is 750 HP or greater.

[Table 1b](#Tbl_1b): Title 30 Texas Administrative Code Chapter 117 (30 TAC Chapter 117), Subchapter B: Combustion Control at Major Industrial, Commercial, and Institutional Sources in Ozone Nonattainment Areas

Unit ID No.:

Enter the identification number (ID No.) for the SRIC engines (maximum 10 characters) as listed on Form OP-SUM (Individual Unit Summary).

SOP/GOP Index No.:

SOP applicants should indicate the SOP index number for the unit or group of units (maximum 15 characters consisting of numeric, alphanumeric characters, and/or dashes prefixed by a code for the applicable regulation [i.e., 60KB XXXX]). GOP applicants should indicate the appropriate GOP index number in this column from the applicable GOP table (SSS‑FF-XXX). Applicants should complete all applicable GOP attribute information before determining the GOP index number. For additional information relating to SOP index numbers, please go to the TCEQ website at [www.tceq.texas.gov/permitting/air/guidance/titlev/tv\_fop\_guidance.html](https://www.tceq.texas.gov/permitting/air/guidance/titlev/tv_fop_guidance.html).

NOx Emission Limitation:

Title 30 TAC Chapter 117 provides several methods to be in compliance with the applicable NOx emission specifications of 30 TAC Chapter 117. Select one of the following options. Enter the code on the form.

For GOP applications:

**Code Description**

105 Title 30 TAC §§ 117.105(a)(1), (a)(3), (d), or (e) [relating to Emission Specifications for Reasonably Available Control Technology] (use for SRIC engines in the Beaumont/Port Arthur Ozone Nonattainment Area) 410 A Title 30 TAC § 117.410(a) [relating to Emission Specifications for Eight-Hour Attainment Demonstration] (use for SRIC engines in the Dallas/Fort Worth Eight-Hour Ozone Nonattainment Area)

410A Title 30 TAC § 117.410(a)(4) [relating to Emission Specifications for Eight-Hour Attainment Demonstration] (use for SRIC engines in the Dallas/Fort Worth Eight-Hour Ozone Nonattainment Area)

310D Title 30 TAC § 117.310(d)(3) [relating to Emission Specifications for Attainment Demonstration] (use for SRIC engines in the Houston/Galveston/Brazoria Ozone Nonattainment Area)

405B Title 30 TAC § 117.405(b)(2)(A) [relating to Emission Specifications for Reasonably Available Control Technology (RACT) gas-fired rich-burn engines used in Wise County]

WS4C White Superior four-cycle lean-burn engine is complying with Title 30 TAC § 117.405(b)(2)(B)(i)

C2C Clark two-cycle lean-burn engine is complying with Title 30 TAC § 117.405(b)(2)(B)(ii)

FM2C Fairbanks Morse MEP two-cycle lean-burn engine is complying with Title 30 TAC § 117.405(b)(2)(B)(iii)

WSE All other lean-burn engines located in Wise County complying with Title 30 TAC § 117.405(b)(2)(B)(iv)

For SOP applications:

For SRIC engines located in the Beaumont/Port Arthur Ozone Nonattainment Areas:

**Code Description**

105 Title 30 TAC §§ 117.105(a)(1), (a)(3), (d) or (e) [relating to Emissions Specifications for Reasonably Available Control Technology]

APES Engine is complying with an Alternative Plant-Wide Emissions Specification under Title 30 TAC § 117.115(a)

ACSS Engine is complying with an Alternative Case Specific Specification under Title 30 TAC § 117.125(a)

SC Engine is complying with a Source Cap under Title 30 TAC § 117.123(a)

For SRIC engines located in the Houston/Galveston/Brazoria Ozone Nonattainment Area:

**Code Description**

310D Title 30 TAC §§ 117.310(d)(3) and 117.310(a)(9) [relating to mass emissions cap and trade in Chapter 101, Subchapter H, Division 3, and Emission Specifications for Attainment Demonstration]

ACF Engine is complying with an annual capacity factor specification under Title 30 TAC §§ 117.310(d)(3) and 117.310(a)(17)

For SRIC engines located in the Dallas/Fort Worth Eight-Hour Ozone Nonattainment Area:

**Code Description**

410A Title 30 TAC § 117.410(a)(4) [relating to Emission Specifications for Eight-Hour Attainment Demonstration]

405B Title 30 TAC § 117.405(b)(2)(A) [relating to Emission Specifications for Reasonably Available Control Technology (RACT) gas fired rich burn engines used in Wise County]

ACF Engine is complying with an annual capacity factor specification under Title 30 TAC § 117.410(a)(14)

SC Engine is complying with a Source Cap under Title 30 TAC § 117.423(a)

WS4C White Superior four-cycle-lean-burn engine is complying with Title 30 TAC § 117.405(b)(2)(B)(i)

C2C Clark two-cycle-lean-burn engine is complying with Title 30 TAC § 117.405(b)(2)(B)(ii)

FM2C Fairbanks Morse MEP two-cycle-lean-burn engine is complying with Title 30 TAC § 117.405(b)(2)(B)(iii)

WSE All other -lean-burn engines located in Wise County complying with Title 30 TAC § 117.405(b)(2)(B)(iv)

* Complete “23C-Option” only if “NOx Emission Limitation” is “SC.”

23C-Option:

Select one of the following § 117.123(c)(1) or 423(c)(1) options for monitoring. Enter the code on the form.

**Code Description**

23C-A CEMS and a totalizing fuel flow meter per § 117.123(c)(1)(A) or § 117.423(c)(1)(A).

23C-B PEMS and a totalizing fuel flow meter per § 117.123(c)(1)(B) or § 117.423(c)(1)(B).

23C-C Rate measured by hourly emission rate testing per § 117.123(c)(1)(C) or § 117.423(c)(1)(C).

* Complete “30 TAC Chapter 116 Limit” only if “NOx Emission Limitation” is “105.”

30 TAC Chapter 116 Limit:

Select one of the following descriptions for the 30 TAC Chapter 116 permit limit. Enter the code on the form.

For units having a 30 TAC Chapter 116 permit in effect on June 9, 1993:

**Code Description**

93Y NOx emission limit in 30 TAC § 117.105 is greater than the NOx emission limit in a 30 TAC Chapter 116 permit

93N NOx emission limit in 30 TAC § 117.105 is not greater than the NOx emission limit in a 30 TAC Chapter 116 permit

For units placed into service after June 9, 1993 and prior to the final compliance date specified in 30 TAC §§ 117.9000 or 117.9020(1) as a functionally identical replacement for an existing unit, or group of units, and limited to the cumulative maximum rated capacity of the units replaced:

**Code Description**

95Y Emission limit in 30 TAC §§ 117.105 or is greater than the NOx emission limit in any 30 TAC Chapter 116 permit issued after June 9, 1993

95N Emission limit in 30 TAC §§ 117.105 or is not greater than the NOx emission limit in any 30 TAC Chapter 116 permit issued after June 9, 1993

* Complete “EGF System Cap Unit” only if located in the Houston/Galveston/Brazoria Ozone Nonattainment Area.

EGF System Cap Unit:

Enter “YES” if the engine is used as an electric generating facility to generate electricity for sale to the electric grid. Otherwise, enter “NO.”

16TUnits with electric output entirely dedicated to industrial customers or that generate electricity primarily for internal use are not considered as electric generating facilities generating electricity for sale to the electric grid and are not subject to the system cap requirements of 30 TAC § 117.320. “Entirely dedicated” may include up to two weeks per year of service to the electric grid when the industrial customer’s load sources are not operating. Units generating electricity primarily for internal use are those that have previously or will transfer generated electricity to a utility power distribution system at a rate less than 3.85% of actual electrical generation.

NOx Averaging Method:

Select one of the following options for the method used to comply with the applicable emission limitation. Enter the code on the form.

**Code Description**

30D Complying with the applicable emission limit using a 30-day rolling average

1HR Complying with the applicable emission limits using a block one-hour average

NOx Reduction:

Select one of the following NOx reduction options. Enter the code on the form.

**Code Description**

WATER Water or steam injection

NSCR Nonselective catalytic reduction

POST1 Post combustion control technique with urea or ammonia injection

POST2 Post combustion control technique with chemical reagent other than urea or ammonia

OTHER Other post combustion control method

NONE No NOx reduction

NOx Monitoring System:

Select the appropriate code to indicate the type of monitoring system used.

For units without a monitoring system:

**Code Description**

MERT Maximum emission rate testing in accordance with 30 TAC § 117.8000

For all other units:

**Code Description**

CEMS Continuous emissions monitoring system

PEMS Predictive emissions monitoring system

75ARC CEMS used to comply with 40 CFR Part 75 (pertaining to acid rain) (for SOP applications only)

75ARP PEMS used to comply with 40 CFR Part 75 (pertaining to acid rain) (for SOP applications only)

* **Continue only if application type is SOP.**

[Table 1c:](#Tbl_1c) Title 30 Texas Administrative Code Chapter 117 (30 TAC Chapter 117), Subchapter B: Combustion Control at Major Industrial, Commercial, and Institutional Sources in Ozone Nonattainment Areas

Unit ID No.:

Enter the identification number (ID No.) for the SRIC engines (maximum 10 characters) as listed on Form OP-SUM (Individual Unit Summary).

SOP/GOP Index No.:

SOP applicants should indicate the SOP index number for the unit or group of units (maximum 15 characters consisting of numeric, alphanumeric characters, and/or dashes prefixed by a code for the applicable regulation [i.e., 60KB XXXX]). GOP applicants should indicate the appropriate GOP index number in this column from the applicable GOP table (SSS‑FF-XXX). Applicants should complete all applicable GOP attribute information before determining the GOP index number. For additional information relating to SOP and numbers, please go to the TCEQ website at [www.tceq.texas.gov/permitting/air/guidance/titlev/tv\_fop\_guidance.html](https://www.tceq.texas.gov/permitting/air/guidance/titlev/tv_fop_guidance.html).

Fuel Flow Monitoring:

Select one of the following options to indicate how fuel flow is monitored. Enter the code on the form.

**Code Description**

X40A Fuel flow is with a totalizing fuel flow meter per 30 TAC §§ 117.140(a), 117.340(a) or 117.440(a)

X40A2-A Unit operates with a NOx and diluents CEMS and monitors stack exhaust flow per 30 TAC §§ 117.140(a)(2)(A), 117.340(a)(2)(A) or 117.440(a)(2)(A)

X40A2-B Unit vents to a common stack with a NOx and diluents CEMS and uses a single totalizing fuel flow meter per 30 TAC §§ 117.140(a)(2)(B), 117.340(a)(2)(B) or 117.440(a)(2)(B).

X40A2-C The unit is a diesel engine operating with a run time meter and using monthly fuel use records maintained for each engine per 30 TAC §§ 117.340(a)(2)(C) or 117.440(a)(2)(C) [Houston/Galveston/Brazoria or Dallas/Fort Worth Eight-Hour Ozone Nonattainment Areas only]

X40A2-D The unit is equipped with a continuous monitoring system that continuously monitors horsepower and hours of operation per 30 TAC §§ 117.140(a)(2)(D), 117.340(a)(2)(D) or 117.440(a)(2)(D).

* Complete “CO Emission Limitation” only for SOP applications.

CO Emission Limitation:

Title 30 TAC Chapter 117 provides several methods to be in compliance with the applicable CO emission specifications of 30 TAC Chapter 117. Select one of the following options. Enter the code on the form.

For SRIC engines located in the Beaumont/Port Arthur Ozone Nonattainment Areas:

**Code Description**

105 Title 30 TAC § 117.105(d) or (e) [relating to Emissions Specifications for Reasonably Available Control Technology]

ACSS Engine is complying with an Alternative Case Specific Specification under 30 TAC § 117.125(a)

For SRIC engines located in the Houston/Galveston/Brazoria Ozone Nonattainment Area:

**Code Description**

310C Title 30 TAC § 117.310(c)(1) 400 ppmv option

310CG Title 30 TAC § 117.310(c)(1) 3 g/HP-hr option

ACSS Engine is complying with an Alternative Case Specific Specification under 30 TAC § 117.325(a)

For SRIC engines located in the Dallas/Fort Worth Eight-Hour Ozone Nonattainment Area:

**Code Description**

410C Title 30 TAC § 117.410(c)(1) [relating to Emission Specifications for Eight-Hour Attainment Demonstration]

405D Title 30 TAC § 117.405(d)(1) [relating to Emission Specifications for Eight-Hour Attainment Demonstration]

ACSS Engine is complying with an Alternative Case Specific Specification under 30 TAC § 117.425(a)

CO Averaging Method:

Select one of the following options for the method used to comply with the applicable emission limitation. Enter the code on the form.

**Code Description**

30D Complying with the applicable emission limit using a 30-day rolling average

1HR Complying with the applicable emission limits using a block one-hour average

CO Monitoring System:

Select one of the following options to indicate how the unit is monitored for CO exhaust emissions. Enter the code on the form.

**Code Description**

CEMS Continuous emissions monitoring system complying

PEMS Predictive emissions monitoring system complying

OTHER Other than CEMS or PEMS

* Complete “NHR3R Emission Limitation” only for SOP applications and only if “NOx Reduction” is “POST1.”

NHR3R Emission Limitation:

Title 30 TAC Chapter 117 provides several methods to be in compliance with the applicable NHR3R emission specifications of 30 TAC Chapter 117. Select one of the following options. Enter the code on the form.

For SRIC engines located in the Beaumont/Port Arthur Ozone Nonattainment Areas:

**Code Description**

105 Title 30 TAC §§ 117.105(g) [relating to Emissions Specifications for Reasonably Available Control Technology]

ACSS Engine is complying with an Alternative Case Specific Specification under 30 TAC § 117.125(a)

For SRIC engines located in the Houston/Galveston/Brazoria Ozone Nonattainment Area:

**Code Description**

310C Title 30 TAC § 117.310(c)(2) [relating to Emission Specifications for Attainment Demonstration]

ACSS Engine is complying with an Alternative Case Specific Specification under 30 TAC § 117.325(a)

For SRIC engines located in the Dallas/Fort Worth Eight-Hour Ozone Nonattainment Area:

**Code Description**

410C Title 30 TAC § 117.410(c)(2) [relating to Emission Specifications for Attainment Demonstration] (use for engines in the Dallas/Fort Worth Eight-Hour Ozone Nonattainment Area

405D Title 30 TAC § 117.405(d)(2) [relating to Emission Specifications for Attainment Demonstration] (use for engines in Wise County in the Dallas/Fort Worth Eight-Hour Ozone Nonattainment Area

ACSS Engine is complying with an Alternative Case Specific Specification under 30 TAC § 117.425(a)

16TNote: If using some other alternative, such as an alternate reasonably available control technology, alternate means of control, or emission reduction credit, the type of alternate used will need to be explained in a cover letter or some other attachment to the permit application.

NHR3R Monitoring:

Select one of the following options to indicate how the unit is monitored for NHR3R emissions. Enter the code on the form.

**Code Description**

CEMS Continuous emissions monitoring system

PEMS Predictive emissions monitoring system

MBAL Mass balance

OXY Oxidation of ammonia to nitric oxide (NO)

STUBE Stain tube

[Table 2a](#Tbl_2a): Title 40 Code of Federal Regulations Part 63 (40 CFR Part 63), Subpart ZZZZ: National Emission Standards for Hazardous Air Pollutants for Stationary Reciprocating Internal Combustion Engines

* Complete this table for all stationary Reciprocating Internal Combustion Engines (RICE) in GOP and SOP applications that are not being tested at a stationary RICE test cell:

Unit ID No.:

Enter the identification number (ID No.) for the stationary reciprocating internal combustion engine unit (maximum 10 characters) as listed on Form OP-SUM (Individual Unit Summary).

SOP/GOP Index No.:

Site operating permit (SOP) applicants should indicate the SOP index number for the unit or group of units (maximum 15 characters consisting of numeric, alphanumeric characters, and/or dashes prefixed by a code for the applicable regulation [i.e., 60KB-XXXX]). GOP applicants should indicate the appropriate GOP index number in this column from the applicable GOP table (SSS-FF-XXX). Applicants should complete all applicable GOP attribute information before determining the GOP index number. For additional information relating to SOP index numbers, please go to the TCEQ website at [www.tceq.texas.gov/permitting/air/guidance/titlev/tv\_fop\_guidance.html](https://www.tceq.texas.gov/permitting/air/guidance/titlev/tv_fop_guidance.html).

HAP Source:

Select one of the following options to describe the HAP source classification

**Code Description**

MAJOR The site is a major source of hazardous air pollutants as defined in 40 CFR § 63.2

AREA The site is an area source of hazardous air pollutants as defined in 40 CFR § 63.2

Brake HP:

Select one of the following options to indicate the brake horsepower (HP). Enter the code on the form.

**Code Description**

100- Stationary RICE with a brake HP less than 100 HP

100-250 Stationary RICE with a brake HP greater than or equal to 100 and less than 250 HP

250-300 Stationary RICE with a brake HP greater than or equal to 250 HP and less than 300 HP

300-500 Stationary RICE with a brake HP greater than or equal to 300 HP and less than or equal to 500 HP

500+ Stationary RICE with a brake HP greater than 500 HP

5000+ Stationary RICE with a brake HP of 5,000 HP or greater (use only for 4 stroke spark ignited richburn RICE)

Construction/Reconstruction Date:

Select one of the following options that describe the date of commencement of the most recent construction or reconstruction. Enter the code on the form.

**Code Description**

02- Commenced construction or reconstruction before December 19, 2002

02-06 Commenced construction or reconstruction on or after December 19, 2002, but before June 12, 2006

06+ Commenced construction or reconstruction on or after June 12, 2006

* Complete “Nonindustrial Emergency Engine” only if “HAP Source” is “AREA” and “Construction/Reconstruction Date” is “02-” or “02‑06.”

Nonindustrial Emergency Engine:

Enter “YES” if the Stationary RICE is defined in 40 CFR §63.6675 as a residential emergency RICE, a commercial emergency RICE, or an institutional emergency RICE. Otherwise, enter “NO.”

* **Do not continue if “HAP Source” is “AREA” and:**
* “Construction/Reconstruction Date” is “06+;” or
* “Nonindustrial Emergency Engine” is “YES.”

Service Type:

Select one of the following options that describe the type of service the stationary RICE is used for. Enter the code on the form. Note: The provisions of 40 CFR §63.6640(f)(2)(ii) and (f)(2)(iii) for emergency engines have been vacated by the U.S. Court of Appeals for the District of Columbia Circuit.

**Code Description**

FUEL Combusts landfill or digester gas equivalent to 10 % or more of the gross heat input on an annual basis

LIM Limited use

EMER-A Emergency use where the RICE does not operate as specified in 40 CFR §63.6640(f)(2)(ii) and (iii) or does not operate as specified in 40 CFR §63.6640(f)(4)(ii)

EMER-B Emergency use where the RICE operates for the purpose specified in 40 CFR §63.6640(f)(4)(ii) (Use only for RICE located at an area source)

BLSTRT Black Start Use (use only for existing RICE, less than 500 HP, located at a major source; or existing RICE located at an area source)

NORMAL Normal Use

* **Do not continue if “HAP Source” is “MAJOR” and:**
* “Brake HP” is “500+” and “Service Type” is “LIM” or “EMER-A;” or
* “Brake HP” is “500+” and “Construction/Reconstruction Date” is “02-,” and “Service Type” is “FUEL;” or
	+ - “Construction/Reconstruction Date” is “06+” and “Brake HP” is “100-,” “100-250,” “250-300,” or “300‑500” and “Service Type” is “FUEL,” “LIM,” or “EMER-A,” or “EMER-B”.

Stationary Rice Type:

Select one of the following options that describe the type of stationary RICE that you own or operate. Enter the code on the form.

**Code Description**

2SLB 2 stroke spark ignited lean burn engine

4SLB 4 stroke spark ignited lean burn engine

4SLBR remote 4 stroke spark ignited lean burn engine (use only for existing non-emergency, non-black start 4SLB with a site rating greater than 500 HP, located at an area source, that is a remote stationary RICE as defined in 40 CFR § 63.6675)

4SRB 4 stroke spark ignited rich burn engine

4SRBR remote 4 stroke spark ignited rich burn engine (use only for existing non-emergency, non-black start 4SRB with a site rating greater than 500 HP, located at an area source, that is a remote stationary RICE as defined in 40 CFR § 63.6675)

CI Compression ignition engine (use only for CI engines not meeting § 63.6603(d) or § 63.6603(e))

TIER1/2 Existing non-emergency CI RICE with a site rating of more than 300 HP located at an area source that is certified to the Tier 1 or Tier 2 emission standards electing to comply with the management practices as specified in 40 CFR § 63.6603(d)

TIER3 Existing non-emergency CI RICE with a site rating of more than 300 HP located at an area source that is certified to the Tier 3 (Tier 2 for engines above 560 kilowatt (kW)) emission standards electing to comply with 40 CFR Part 60, Subpart IIII

* **Do not continue if “HAP Source” is “MAJOR” and “Construction/Reconstruction Date” is “06+” and “Service Type” is “NORMAL,” and:**
* “Brake HP” is “100-,” “100-250,” “250-300,” or “300‑500” and “Stationary RICE Type” is “2SLB,” “4SRB,” or “CI;” or
* “Brake HP” is “100-” or “100-250” and “Stationary RICE Type” is “4SLB.”
* **Do not continue if “HAP Source” is “MAJOR” and “Construction/Reconstruction Date” is “02-” and “Brake HP” is “500+” and “Stationary RICE Type” is “2SLB” or “4SLB.”**
* **Do not continue if “HAP Source” is “MAJOR” and “Construction/Reconstruction Date” is “02-” or “02-06” and:**
* “Service Type” is “BLSTRT,” “EMER-A,” or “EMER-B” and “Brake HP” is “100-,” “100-250,” “250‑300,” or “300‑500;” or
* “Brake HP” is “100-” and “Service Type” is “LIM,” “NORMAL,” or “FUEL.”
* **Do not continue if “HAP Source” is “AREA” and:**
* “Service Type” is “BLSTRT;” or
* “Service Type” is “LIM” or “NORMAL,” and “Stationary RICE Type” is “CI,” and “Brake HP” is “100-,” “100-250,” or “250-300;” or
* “Service Type” is “LIM” or “NORMAL,” and “Stationary RICE Type” is “2SLB;” or
* “Service Type” is “LIM” or “NORMAL,” and “Stationary RICE Type” is “4SRB” or “4SLB” and “Brake HP” is “100-,” “100-250,” “250-300,” or “300-500;” or
* “Brake HP” is “500+,” and “Service Type” is “LIM” or “NORMAL,” and “Stationary RICE Type” is “4SLBR” or “4SRBR.;” or
* “Service Type” is “EMER-A,” and “Stationary RICE Type” is “CI,” and “Brake HP” is “100-,” “100‑250,” “250-300,” “300-500,” or “500+;” or
* “Service Type” is “EMER-A” or “EMER-B,” and “Stationary RICE Type” is “2SLB” or “4SLB” or “4SRB,” and “Brake HP” is “100-,” “100-250,” “250-300,” “300-500,” or “500+;” or
* “Service Type” is “FUEL.”
* **Do not continue if “HAP Source” is “MAJOR” and Construction/Reconstruction Date” is “02-,” 02-06,” or “06+,” and “Brake HP” is “500+,” and “Stationary RICE Type” is “2SLB,” “4SRB,” or “4SLB,” and “Service Type” is “EMER-B.”**
* “**HAP Source is “MAJOR” and Construction/Reconstruction Date” is “02-,” 02-06,” or “06+,” and “Brake HP” is “500+,” and “Stationary RICE Type” is “CI,” and “Service Type” is “EMER-B,” complete “Displacement” on Table 2b only. No further information is required.**
* **HAP Source” is “AREA” and Construction/Reconstruction Date” is “02-” or “02-06,” and “Brake HP” is “100-250” or “100-250” or “250-300” or “300-500” or “500+,” and “Stationary RICE Type” is “CI,” and “Service Type” is “EMER-B,” complete “Displacement” on Table 2b only. No further information is required**.

[**Table 2b**](#Tbl_2b)**: Title 40 Code of Federal Regulations Part 63 (40 CFR Part 63), Subpart ZZZZ: National Emission Standards for Hazardous Air Pollutants for Stationary Reciprocating Internal Combustion Engines**

Unit ID No.:

Enter the identification number (ID No.) for the stationary reciprocating internal combustion engine unit (maximum 10 characters) as listed on Form OP-SUM (Individual Unit Summary).

SOP/GOP Index No.:

Site operating permit (SOP) applicants should indicate the SOP index number for the unit or group of units (maximum 15 characters consisting of numeric, alphanumeric characters, and/or dashes prefixed by a code for the applicable regulation [i.e., 60KB-XXXX]). GOP applicants should indicate the appropriate GOP index number in this column from the applicable GOP table (SSS-FF-XXX). Applicants should complete all applicable GOP attribute information before determining the GOP index number. For additional information relating to SOP index numbers, please go to the TCEQ website at [www.tceq.texas.gov/permitting/air/guidance/titlev/tv\_fop\_guidance.html](https://www.tceq.texas.gov/permitting/air/guidance/titlev/tv_fop_guidance.html).

* Complete “Manufacture Date” only if “Stationary RICE Type” is “4SLB” and “Brake HP” is “250-300” or “300-500” and “Construction/Reconstruction Date” is “06+.”

Manufacture Date:

Enter “YES” if the stationary RICE was manufactured on or after January1, 2008. Otherwise, enter “NO.”

* **Do not continue if “Manufacture Date” is “NO.”**
* Complete “Operating Hours” only if “HAP Source” is “AREA” and “Stationary RICE Type” is “4SLB” or “4SRB,” and “Brake HP” is “500+.”

Operating Hours:

Enter “YES” if the stationary RICE is operated less than 24 hours per calendar year. Otherwise, enter “NO.”

* **Do not continue if “Operating Hours” is “YES.”**

Different Schedule:

Enter “YES” if the Administrator has approved a different schedule for the submission of reports under 40 CFR § 63.10(a). Otherwise, enter “NO.”

* **Do not continue if “HAP Source” is “MAJOR” and “Service Type” is “FUEL.”**

Emission Limitation:

Select one of the following options for compliance with the emission limitations. Enter the code on the form.

**Code Description**

76+ Reducing formaldehyde emission by 76% or greater (use for richburn, spark ignited engines)

76+THC Complying with reducing formaldehyde emissions by 76% or greater by testing for THC instead of formaldehyde. Average reduction of THC emissions is 30% or greater. (use for non‑emergency 4SRB RICE)

REDCO Reducing carbon monoxide emissions from the stationary RICE

LIMCO Limiting the concentration of carbon monoxide in the stationary RICE exhaust

CONC Limiting formaldehyde concentration from the stationary RICE exhaust

REDTHC Reducing THC emissions from the stationary RICE

* **Continue only for SOP applications.**
* Complete “Displacement” and “Crankcase” only if “Service Type” is “NORMAL” or “LIM,” “Stationary RICE Type” is “CI,” “Brake HP” is “300-500” or “500+” and “Construction/Reconstruction Date” is

“02‑” or “02-06.”

* Complete “Displacement” only if “Service Type” is “EMER-B,” “Stationary RICE Type is “CI,” “Brake HP” is “100-250,” “250-300,” “300-500” or “500+” and “Construction/Reconstruction Date” is “02-,”

“02-06” or “06+.”

Displacement:

Enter “YES” if the stationary CI RICE has a displacement of less than 30 liters per cylinder and uses diesel fuel. Otherwise, enter “NO.”

[Table 2c](#Tbl_2c): Title 40 Code of Federal Regulations Part 63 (40 CFR Part 63), Subpart ZZZZ: National Emission Standards for Hazardous Air Pollutants for Stationary Reciprocating Internal Combustion Engines

Unit ID No.:

Enter the identification number (ID No.) for the stationary reciprocating internal combustion engine unit (maximum 10 characters) as listed on Form OP-SUM (Individual Unit Summary).

SOP/GOP Index No.:

Site operating permit (SOP) applicants should indicate the SOP index number for the unit or group of units (maximum 15 characters consisting of numeric, alphanumeric characters, and/or dashes prefixed by a code for the applicable regulation [i.e., 60KB-XXXX]). GOP applicants should indicate the appropriate GOP index number in this column from the applicable GOP table (SSS-FF-XXX). Applicants should complete all applicable GOP attribute information before determining the GOP index number. For additional information relating to SOP index numbers, please go to the TCEQ website at [www.tceq.texas.gov/permitting/air/guidance/titlev/tv\_fop\_guidance.html](https://www.tceq.texas.gov/permitting/air/guidance/titlev/tv_fop_guidance.html).

Crankcase:

Enter “YES” if the stationary CI RICE is equipped with a closed crankcase ventilation system. Otherwise, enter “NO.”

Performance Test:

Enter “YES” if a performance test has been previously conducted that meets the conditions in 40 CFR § 63.6610(d)(1)-(5) or § 63.6612(b)(1)-(4). Otherwise, enter “NO.”

Control Technique:

Select one of the following options to indicate the type of control device used. Enter the code on the form.

For 4 strokes spark ignited rich burn engines (4 SRB):

**Code Description**

NSCR Non-selective catalytic reduction

OTHER1 Control technique other than non-selective catalytic reduction

For 2 strokes spark ignited lean burn engines (2 SLB), 4 strokes spark ignited lean burn engines (4 SLB), and compression ignition engines (CI):

**Code Description**

OXCAT Oxidation catalyst

OTHER2 Control technique other than an oxidation catalyst

* Complete “Operating Limits” only if “Control Technique” is “OTHER1” or “OTHER2.”

Operating Limits:

Enter “YES” if the Administrator has been petitioned to establish operating limitations during the initial performance test. Otherwise, enter “NO.”

Monitoring System:

Select one of the following options to indicate the type of monitoring used. Enter the code on the form.

**Code Description**

CEMS Continuous emission monitoring system

CPMS Continuous parameter monitoring system

OTHER The owner or operator has chosen to use a monitoring system that is not a CEMS or CPMS.

SHUT1 The owner or operator has installed a system to shutdown the engine when the catalyst inlet temperature exceeds 1350°F (use only for existing non-emergency, non-remote 4SLB engines greater than 500 brake HP located at an area source)

SHUT2 The owner or operator has installed a system to shutdown the engine when the catalyst inlet temperature exceeds 1250°F (use only for existing non-emergency, non-remote 4SRB engines greater than 500 brake HP located at an area source)

[Table 3](#Tbl_3): Title 30 Texas Administrative Code Chapter 117 (30 TAC Chapter 117),

**Subchapter E: Multi-Region Combustion Control, Division 4: East Texas Combustion**

* Complete Table 3 only for stationary, gas-fired reciprocating internal combustion engines.
* Complete Table 3 only for facilities located in Anderson, Brazos, Burleson, Camp, Cass, Cherokee, Franklin, Freestone, Gregg, Grimes, Harrison, Henderson, Hill, Hopkins, Hunt, Lee, Leon, Limestone, Madison, Marion, Morris, Nacogdoches, Navarro, Panola, Rains, Robertson, Rusk, Shelby, Smith, Titus, Upshur, Van Zandt, and Wood Counties.

Unit ID No.:

Enter the identification number (ID No.) for the stationary reciprocating internal combustion engine unit (maximum 10 characters) as listed on Form OP-SUM (Individual Unit Summary).

SOP/GOP Index No.:

Site operating permit (SOP) applicants should indicate the SOP index number for the unit or group of units (maximum 15 characters consisting of numeric, alphanumeric characters, and/or dashes prefixed by a code for the applicable regulation [i.e., 60KB-XXXX]). GOP applicants should indicate the appropriate GOP index number in this column from the applicable GOP table (SSS-FF-XXX). Applicants should complete all applicable GOP attribute information before determining the GOP index number. For additional information relating to SOP index numbers, please go to the TCEQ website at [www.tceq.texas.gov/permitting/air/guidance/titlev/tv\_fop\_guidance.html](https://www.tceq.texas.gov/permitting/air/guidance/titlev/tv_fop_guidance.html).

Unit Type:

Select one of the following options that describes the unit type. Enter the code on the form.

**Code Description**

240- The engine has a maximum rated horsepower capacity less than 240 HP.

RESEARCH The engine is use for research and testing.

PERFV The engine is used for purposes of performance verification and testing.

START The engine is used solely to power other engines or gas turbines during startup.

EMERG The engine is operated exclusively in emergency situations, except that operation for testing or maintenance purposes is allowed for up to 100 hours per year, based on a rolling 12-month average

DISASTER The engine is used in response to and during the existence of any officially declared disaster or state of emergency.

AG The engine is used directly and exclusively by the owner or operator for agricultural operations necessary for the growing of crops or raising of fowl or animals.

DIESEL The engine is a diesel engine.

DUAL The engine is a dual-fuel engine.

LEANBN The engine is a gas-fired lean burn engine

NONE The unit does not qualify for any exemptions under the rule.

* **Continue only if “Unit Type” is “NONE.”**

Horsepower Rating:

Select one of the following options to indicate the horsepower (HP). Enter the code on the form.

**Code Description**

500- Stationary gas-fired rich-burn RICE with a HP less than 500 HP.

500+ Stationary gas-fired rich-burn RICE with a HP equal to or greater than 500 HP.

* Complete “Landfill” only if “Horsepower Rating” is “500+.”

Landfill:

Enter “YES” if the gas-fired rich-burn engine is fired on landfill gas. Otherwise, enter “NO.”

Control Operations:

Select one of the following options to indicate NOx operational control requirements. Enter the code on the form.

**Code Description**

POST1 Post combustion control technique with urea or ammonia injection

POST2 Post combustion control technique with chemical reagent other than urea or ammonia

NSCR The engine is controlled with nonselective catalytic reduction.

NONE The engine is not using any of the above control operations.

NOx and OR2R Monitoring:

Select one of the following options to indicate NOx and OR2R monitoring used. Enter the code on the form.

**Code Description**

CEMSNOX The engine is using a CEMS to monitor NOx emissions

PEMSNOX The engine is using a PEMS to monitor NOx emissions.

CEMSBOTH The engine is using a CEMS to monitor both NOx and OR2R emissions.

NONE The engine is not using any of the above methods (unit is complying with § 117.3330(b)(3) monitoring).

Ammonia Use:

Enter “YES” if urea or ammonia injection is used to control NOx emissions. Otherwise, enter “NO.”

* **Continue only if “Ammonia Use” is “YES**.”

NHR3R Emission Limitation:

Title 30 TAC Chapter 117 provides two methods to be in compliance with the applicable NHR3R limitation standards listed in 30 TAC Chapter 117, Subchapter E. Select one of the following options. Enter the code on the form.

**Code Description**

3310 Title 30 TAC § 117.3310(e) [relating to Emission Specifications for Eight-Hour Attainment Demonstration]

ACSS Unit is complying with an Alternative Case Specific Specification under 30 TAC § 117.3325

Ammonia Monitoring:

Select one of the following options that describes the ammonia monitoring used. Enter the code on the form.

**Code Description**

CEMS A continuous emissions monitoring system is used to monitor ammonia emissions.

PEMS A parametric emissions monitoring system is used to monitor ammonia emissions.

MBAL Mass balance

OXY Oxidation of ammonia to nitric oxide (NO)

STUBE Stain tube

[Table 4a](#Tbl_4a): Title 40 Code of Federal Regulations Part 60 (40 CFR Part 60), Subpart JJJJ: Standards of Performance for Stationary Spark Ignition Internal Combustion Engines

Unit ID No.:

Enter the identification number (ID No.) for the stationary spark ignited internal combustion engine unit (maximum 10 characters) as listed on Form OP-SUM (Individual Unit Summary).

SOP/GOP Index No.:

Site operating permit (SOP) applicants should indicate the SOP index number for the unit or group of units (maximum 15 characters consisting of numeric, alphanumeric characters, and/or dashes prefixed by a code for the applicable regulation [i.e., 60KB-XXXX]). GOP applicants should indicate the appropriate GOP index number in this column from the applicable GOP table (SSS-FF-XXX). Applicants should complete all applicable GOP attribute information before determining the GOP index number. For additional information relating to SOP index numbers, please go to the TCEQ website at [www.tceq.texas.gov/permitting/air/guidance/titlev/tv\_fop\_guidance.html](https://www.tceq.texas.gov/permitting/air/guidance/titlev/tv_fop_guidance.html).

Construction/Reconstruction/Modification Date:

Enter “YES” if you own or operate a stationary spark ignition (SI) internal combustion engine (ICE) that commenced construction, reconstruction, or modification after June 12, 2006.

* **Do not continue if “Construction/Reconstruction/Modification Date” is “NO.”**

Test Cell:

Enter “YES” if the SI ICE is being tested at an engine test cell/stand. Otherwise, enter “NO.”

* **Do not continue if “Test Cell” is “YES.”**

Exemption:

Select one of the following codes if the SI ICE is exempt from the requirements of NSPS JJJJ as described in 40 CFR Part 1068, Subpart C or 40 CFR Parts 90 and 1048. *Owners and operator, as well as manufactures may be eligible to request an exemption for national security.*

**Code Description**

EXEMPT The SI ICE is exempt as described in 40 CFR Part 1068 Subpart C or 40 CFR Parts 90 and 1048, OR due to national security

NONE The SI ICE is not exempt

* **Do not continue if “Exemption” is “EXEMPT.”**

Temporary Replacement:

Enter “YES” if the SI ICE is acting as a temporary replacement and is located at a stationary source for less than 1 year and has been properly certified to the standards that would be applicable to such engines under the appropriate non-road engine provisions. Otherwise, enter “NO.”

* **Do not continue if “Temporary Replacement” is “YES.**”

Horsepower:

Select one of the following options to indicate the maximum engine power in horsepower (HP). Enter the code on the form.

For SI ICE that are emergency use only

**Code Description**

25-E Maximum engine power less than or equal to 25 HP

25-100E Maximum engine power greater than 25 HP and less than or equal to 100 HP

100-130E Maximum engine power greater than 100 HP and less than 130 HP

130-500E Maximum engine power greater than or equal to 130 HP and less than 500 HP

500+E Maximum engine power greater than or equal to 500 HP

For SI ICE that are non-emergency use only

**Code Description**

25- Maximum engine power less than or equal to 25 HP

25-100 Maximum engine power greater than 25 HP and less than 100 HP

100-500 Maximum engine power greater than or equal to 100 HP and less than 500 HP

500-1350 Maximum engine power greater than or equal to 500 HP and less than 1350 HP

1350+ Maximum engine power greater than or equal to 1350 HP

Fuel:

Select one of the following options to indicate what fuel the SI ICE is using. Enter the code on the form.

**Code Description**

GASO SI ICE that uses gasoline

NATGAS SI ICE that uses natural gas

RBLPG SI ICE that is a rich-burn engine that uses liquefied petroleum gas (LPG)

LBLPG SI ICE that is a lean-burn engine that uses liquefied petroleum gas (LPG)

LAND SI ICE that is a landfill/digester gas engine

WELL SI ICE that is a wellhead gas engine that cannot meet natural gas emission limits (use only for SOP applications and only if you are petitioning the EPA per § 60.4233(g); otherwise use “NATGAS”)

* Complete “AEL No.” only if “FUEL” is “WELL.”

AEL No.:

Enter the date of the Alternative Emission Limit approval letter from the EPA.

* **Do not continue if “Fuel” is “WELL.”**
* Complete “Lean Burn” only if BOTH of the following conditions are met:
* “Fuel” is “NATGAS” or “LAND” or “LBLPG;” and
* “Horsepower” is “500-1350.”

Lean Burn:

Enter “YES” if the SI ICE is a lean-burn engine. Otherwise, enter “NO.”

Commencing:

Select one of the following options to indicate the type of construction the SI ICE is commencing. Enter the code on the form.

**Code Description**

CON SI ICE was newly constructed after 06/12/2006

MOD SI ICE was modified after 06/12/2006 (per §60.14)

RECON SI ICE was reconstructed after 06/12/2006 (per §60.15)

[Table 4b](#Tbl_4b): Title 40 Code of Federal Regulations Part 60 (40 CFR Part 60), Subpart JJJJ: Standards of Performance for Stationary Spark Ignition Internal Combustion Engines

Unit ID No.:

Enter the identification number (ID No.) for the stationary spark ignited internal combustion engine unit (maximum 10 characters) as listed on Form OP-SUM (Individual Unit Summary).

SOP/GOP Index No.:

Site operating permit (SOP) applicants should indicate the SOP index number for the unit or group of units (maximum 15 characters consisting of numeric, alphanumeric characters, and/or dashes prefixed by a code for the applicable regulation [i.e., 60KB-XXXX]). GOP applicants should indicate the appropriate GOP index number in this column from the applicable GOP table (SSS-FF-XXX). Applicants should complete all applicable GOP attribute information before determining the GOP index number. For additional information relating to SOP index numbers, please go to the TCEQ website at [www.tceq.texas.gov/permitting/air/guidance/titlev/tv\_fop\_guidance.html](https://www.tceq.texas.gov/permitting/air/guidance/titlev/tv_fop_guidance.html).

Manufacture Date:

Select one of the following options to indicate the date of manufacture of the SI ICE. Enter the code on the form. Please read each date and be careful in choosing the correct date code as each code is very specific to a certain type of SI ICE.

For SI ICE that is commencing 55TNew Construction Only

For SI ICE that is less than or equal to 25 HP (emergency or non-emergency)

**Code Description**

N25-0708- Date of manufacture is prior to July 1, 2008 (use for any cc)

N25-1211- Date of manufacture is on or after July 1, 2008 to December 31, 2011 (use only for SI ICE that is less than 225cc)

N25-0112+ Date of manufacture is on or after January 1, 2012 (use only for SI ICE that is less than225cc)

N25-1210- Date of manufacture is on or after July 1, 2008 to December 31, 2010 (use only for SI ICE that is greater than or equal to 225cc)

N25-0111+ Date of manufacture is on or after January 1, 2011 (use only for SI ICE that is greater than or equal to 225cc)

For SI ICE that is greater than 25 HP (non-emergency only)

**Code Description**

N0708- Date of manufacture is prior to July 1, 2008 (use only for SI ICE that is less than 500 HP)

N0708+ Date of manufacture is on or after July 1, 2008 (use only for SI ICE that is less than 100 HP)

N08-10 Date of manufacture is on or after July 1, 2008 to December 31, 2010 (use only for SI ICE that is greater than or equal to 100 HP and less than 500 HP)

N0111+ Date of manufacture is on or after January 1, 2011 (use only for SI ICE that is greater than or equal to 100 HP and less than 500 HP)

N0707- Date of manufacture is prior to July 1, 2007 (use only for SI ICE that is greater than or equal to 500 HP; except lean-burn SI ICE greater than or equal to 500 HP and less than 1350 HP)

N0108- Date of manufacture is prior to January 1, 2008 (use only if “Lean Burn” is “YES”)

N07-0610- Date of manufacture is on or after July 1, 2007 to June 30, 2010 (use only for SI ICE that is greater than or equal to 500 HP; except lean-burn SI ICE greater than or equal to 500 HP and less than 1350 HP; as stated in Table 1of 40 CFR 60 Subpart JJJJ)

N08-0610- Date of manufacture is on or after January 1, 2008 to June 30, 2010 (use only if “Lean Burn” is “YES”)

N0710+ Date of manufacture is on or after July 1, 2010 (use only for SI ICE that is greater than or equal to 500HP as stated in Table 1 of 40 CFR 60 Subpart JJJJ)

N08- Date of manufacture is on or after July 1, 2007 to July 1, 2008 (use only if “Fuel” is “GASO” or “RBLPG” and SI ICE is greater than or equal to 500 HP) [as stated in § 60.4243(h)]

N08+ Date of manufacture is on or after July 1, 2008 (use only if “Fuel” is “GASO” or “RBLPG” and SI ICE is greater than or equal to 500 HP) [as stated in § 60.4243(h)]

For SI ICE that is greater than 25 HP (emergency only)

**Code Description**

N0109-E Date of manufacture is prior to January 1, 2009

N0109+E Date of manufacture is on or after January 1, 2009 (use only for SI ICE that is greater than 25 HP and less than 130 HP)

N09-10E Date of manufacture is on or after January 1, 2009 to December 31, 2010 (use only for SI ICE that is greater than or equal to 130 HP and less than 500 HP)

N0111+E Date of manufacture is on or after January 1, 2011 (use only for SI ICE that is greater than or equal to 130 HP and less than 500 HP)

N09-610-E Date of manufacture is on or after January 1, 2009 to June 30, 2010 (use only for SI ICE that is greater than or equal to 500 HP)

N0710+E Date of manufacture is on or after July 1, 2010 (use only for SI ICE that is greater than or equal to 500HP)

For SI ICE that is commencing 55TModification or Reconstruction Only

For SI ICE that is less than or equal to 25 HP (emergency or non-emergency)

**Code Description**

R25-0112- Date of manufacture of SI ICE is prior to January 1, 2012(use only for SI ICE that is less than 225cc)

R25-0112+ Date of manufacture of SI ICE is on or after January 1, 2012(use only for SI ICE that is less than 225cc)

R25-0111- Date of manufacture of SI ICE is prior to January 1, 2011(use only for SI ICE that is greater than or equal to 225cc)

R25-0111+ Date of manufacture of SI ICE is on or after January 1, 2011(use only for SI ICE that is greater than or equal to 225cc)

For SI ICE that is greater than 25 HP (non-emergency only)

**Code Description**

R0708- Date of manufacture is prior to July 1, 2008 (use only for SI ICE that is less than 500 HP)

R0708+ Date of manufacture is on or after July 1, 2008 (use only for SI ICE that is less than 500 HP)

R0707- Date of manufacture is prior to July 1, 2007(use only for SI ICE that is greater than or equal to 500 HP; except lean-burn SI ICE greater than or equal to 500 HP and less than 1350 HP)

R0707+ Date of manufacture is on or after July 1, 2007 (use only for SI ICE that is greater than or equal to 500 HP; except lean-burn SI ICE greater than or equal to 500 HP and less than 1350 HP)

R0108- Date of manufacture is prior to January 1, 2008 (use only if “Lean Burn” is “YES”)

R0108+ Date of manufacture is on or after January 1, 2008 (use only if “Lean Burn” is “YES”)

For SI ICE that is greater than 25 HP (emergency only)

**Code Description**

R0708-E Date of manufacture is prior to July 1, 2008 (use only for SI ICE that is less than 130 HP)

R0708+E Date of manufacture is on or after July 1, 2008 (use only for SI ICE that is less than 130 HP)

R0109-E Date of manufacture is prior to January 1, 2009(use only for SI ICE that is greater than or equal to 130 HP and less than 500 HP)

R09-10E Date of manufacture is on or after January 1, 2009 to December 31, 2010 (use only for SI ICE that is greater than or equal to 130 HP and less than 500 HP)

R0111+E Date of manufacture is on or after January 1, 2011 (use only for SI ICE that is greater than or equal to 130 HP and less than 500 HP)

R09-610-E Date of manufacture is on or after January 1, 2009 to June 30, 2010 (use only for SI ICE that is greater than or equal to 500HP)

R0710+E Date of manufacture is on or after July 1, 2010 (use only for SI ICE that is greater than or equal to 500HP)

* **Do not continue if “Manufacture Date” is “N25-0708-,” “N0708-,” “N0707-,” “N0109‑E,” or “N0108‑.”**
* Complete “Displacement” only if “Horsepower” is “25-” or “25-E.”

Displacement:

Select one of the following options to indicate the engine displacement in cubic centimeters (cc). Enter the code on the form.

**Code Description**

66- Engine displacement is less than 66cc

66-100 Engine displacement is greater than or equal to 66cc and less than 100cc

100-225 Engine displacement is greater than or equal to 100cc and less than 225cc

225+ Engine displacement is greater than or equal to 225cc

* Complete “Certified” only if “Commencing” is “CON.”

Certified:

Enter “YES” if you purchased a certified SI ICE. Otherwise, enter “NO.”

* Complete “Operation” only if “Certified” is “YES.”

Operation:

Enter “YES” if you are operating and maintaining the certified SI ICE and control device according to manufacturer’s written instructions. Otherwise, enter “NO.”

* Complete “Certified Modification” only if “Commencing” is “MOD” or “RECON.”

Certified Modification:

Enter “YES” if you purchased, or otherwise own/operate, a modified/reconstructed SI ICE that is certified. Otherwise, enter “NO.”

Service:

Select one of the following options to indicate what type of service the SI ICE is performing. Enter the code on the form.

**Code Description**

EMERG SI ICE is an emergency engine

NON SI ICE is a non-emergency engine

* Complete “Severe Duty” only if either of the following conditions are met:
* “Fuel” is “GASO” or “RBLPG,” and “Service” is “NON,” and “Horsepower” is greater than 25 HP; or
* “Fuel” is not “GASO” or “RBLPG” and “Service” is “NON,” and “Horsepower” is “25-100.”

Severe Duty:

Enter “YES” if the SI ICE is a severe-duty engine. Otherwise, enter “NO.”

* Complete “Optional Compliance” only if “Horsepower” is “500-1350” or “1350+” and “Fuel” is “GASO” or “RBLPG” and “Manufacture Date” is “N08-”.

Optional Compliance:

Select one of the following options to indicate the optional compliance requirements you are choosing to perform.

**Code Description**

PURCH Choosing to purchase an engine certified according to 40 CFR Part 1048 and install and configure the engine according to manufacturer’s specifications.

RECORD Choosing to keep records as indicated in § 60.4243(h)(1), (h)(2), or (h)(3)

[Table 5a](#Tbl_5a): Title 40 Code of Federal Regulations Part 60 (40 CFR Part 60), Subpart IIII: Standards of Performance for Stationary Compression Ignition Internal Combustion Engines

Unit ID No.:

Enter the identification number (ID No.) for the stationary compression ignition internal combustion engine unit (maximum 10 characters) as listed on Form OP-SUM (Individual Unit Summary).

SOP/GOP Index No.:

Site operating permit (SOP) applicants should indicate the SOP index number for the unit or group of units (maximum 15 characters consisting of numeric, alphanumeric characters, and/or dashes prefixed by a code for the applicable regulation [i.e., 60IIII-XX]). GOP applicants should indicate the appropriate GOP index number in this column from the applicable GOP table (SSS-FF-XXX). Applicants should complete all applicable GOP attribute information before determining the GOP index number. For additional information relating to SOP index numbers, please go to the TCEQ website at [www.tceq.texas.gov/permitting/air/guidance/titlev/tv\_fop\_guidance.html](https://www.tceq.texas.gov/permitting/air/guidance/titlev/tv_fop_guidance.html).

Applicability Date:

Select one of the following options to indicate the construction, reconstruction, or modification date of the stationary compression ignition (CI) internal combustion engine (ICE). Enter the code on the form.

**Code Description**

2005+ Stationary CI ICE commenced construction, reconstruction, or modification after 07/11/2005

2005- Stationary CI ICE commenced construction, reconstruction, or modification on or before 07/11/2005

* **Do not continue if “Applicability Date” is “2005-.”**

Exemptions:

Select one of the following options to indicate which exemption could apply to the CI ICE. Enter the code on the form.

**Code Description**

TEST The CI ICE is being tested at an engine test cell/stand

NATSEC The CI ICE is exempt due to national security

TEMP The CI ICE is acting as a temporary replacement and is located at a stationary source for less than 1 year and has been properly certified to the standards that would be applicable to such engines under the appropriate non-road engine provisions

NONE The CI ICE is not eligible for any of these exemptions

* **Continue only if “Exemptions” is “NONE.”**

Service:

Select one of the following options to indicate what type of service the CI ICE is performing. Enter the code on the form.

**Code Description**

NON CI ICE is a non-emergency engine

EMERG CI ICE is an emergency engine

FIRE CI ICE is a fire-pump engine (an emergency engine certified to National Fire Protection Association requirements)

Commencing:

Select one of the following options to indicate what type of construction occurred after 07/11/2005. Enter the code on the form.

**Code Description**

CON CI ICE was newly constructed after 07/11/2005

MOD CI ICE was modified after 07/11/2005 (per §60.14)

RECON CI ICE was reconstructed after 07/11/2005 (per §60.15)

* Complete “Manufacture Date” only if “Commencing” is “CON.”

Manufacture Date:

Select one of the following options to indicate when the CI ICE was manufactured. Enter the code on the form.

For CI ICE for which “Service” is “NON” or “EMERG”

**Code Description**

0406- Date of manufacture was on or prior to 04/01/2006.

0406+ Date of manufacture was after 04/01/2006.

For CI ICE for which “Service” is “FIRE”

**Code Description**

0706- Date of manufacture was on or prior to 07/01/2006.

0706+ Date of manufacture was after 07/01/2006.

* **Do not continue if “Manufacture Date” is “0406-” or “0706-.”**

[**Table 5b**](#Tbl_5b)**: Title 40 Code of Federal Regulations Part 60 (40 CFR Part 60), Subpart IIII: Standards of Performance for Stationary Compression Ignition Internal Combustion Engines**

Unit ID No.:

Enter the identification number (ID No.) for the stationary compression ignition internal combustion engine unit (maximum 10 characters) as listed on Form OP-SUM (Individual Unit Summary).

SOP/GOP Index No.:

Site operating permit (SOP) applicants should indicate the SOP index number for the unit or group of units (maximum 15 characters consisting of numeric, alphanumeric characters, and/or dashes prefixed by a code for the applicable regulation [i.e., 60IIII-XX]). GOP applicants should indicate the appropriate GOP index number in this column from the applicable GOP table (SSS-FF-XXX). Applicants should complete all applicable GOP attribute information before determining the GOP index number. For additional information relating to SOP index numbers, please go to the TCEQ website at [www.tceq.texas.gov/permitting/air/guidance/titlev/tv\_fop\_guidance.html](https://www.tceq.texas.gov/permitting/air/guidance/titlev/tv_fop_guidance.html).

Diesel:

Select one of the following codes to indicate fuel being used. Enter the code on the form.

**Code Description**

DIESEL Diesel fuel is used

AES Alternative Emission Standard has been approved by the EPA Administrator

* Complete “AES No.” only if “Diesel” is “AES.”

AES No.:

If an AES has been approved by the EPA administrator, enter the corresponding AES unique identifier for each unit (maximum 10 characters). If the unique identifier is unavailable, then enter the date of the AES approval letter in the table column. The unique identifier and/or the date of the approval letter are contained in the Compliance File under the appropriate regulated entity number. Otherwise, leave this column blank.

* **Do not continue if “Diesel” is “AES.”**

Displacement:

Select one of the following options to indicate the displacement of the CI ICE (expressed in liters per cylinder). Enter the code on the form.

**Code Description**

10-CS Displacement is less than 10 liters per cylinder and is a constant-speed engine. (16TUse only if “Service” is “NON” or “EMERG.”16T)

10- Displacement is less than 10 liters per cylinder.

10-15 Displacement is greater than or equal to 10 and less than 15 liters per cylinder.

15-20 Displacement is greater than or equal to 15 and less than 20 liters per cylinder.

20-25 Displacement is greater than or equal to 20 and less than 25 liters per cylinder.

25-30 Displacement is greater than or equal to 25 and less than 30 liters per cylinder.

30+ Displacement is greater than or equal to 30 liters per cylinder.

* Complete “Generator Set” only if “Service” is “NON” and “Displacement” is “10-.”

Generator Set:

Enter “YES” if the CI ICE is a generator set engine. Otherwise, enter “NO.”

* Do not complete “Model Year” if “Displacement” is “30+.”

Model Year:

Select one of the following options to indicate what model year the CI ICE was manufactured in. Enter the code on the form.

**Code Description**

2007- CI ICE was manufactured prior to model year 2007.

2007 CI ICE was manufactured in model year 2007.

2008 CI ICE was manufactured in model year 2008.

2009 CI ICE was manufactured in model year 2009.

2010 CI ICE was manufactured in model year 2010.

2011 CI ICE was manufactured in model year 2011.

2012 CI ICE was manufactured in model year 2012.

2013 CI ICE was manufactured in model year 2013.

2014 CI ICE was manufactured in model year 2014.

2015 CI ICE was manufactured in model year 2015.

2016 CI ICE was manufactured in model year 2016.

2017+ CI ICE was manufactured in model year 2017 or later.

* Complete “Install Date” only if “Displacement” is “30+.”

Install Date:

Select one of the following options to indicate what year the CI ICE was installed. Enter the code on the form.

**Code Description**

2012- The CI ICE was installed prior to 2012.

2012+ The CI ICE was installed in 2012 or later (use only if “Service” is “EMERG” or “FIRE”).

2012-2015 The CI ICE was installed in 2012 through 2015.

2016+ The CI ICE was installed in 2016 or later.

[**Table 5c**](#Tbl_5c)**: Title 40 Code of Federal Regulations Part 60 (40 CFR Part 60), Subpart IIII: Standards of Performance for Stationary Compression Ignition Internal Combustion Engines**

Unit ID No.:

Enter the identification number (ID No.) for the stationary compression ignition internal combustion engine unit (maximum 10 characters) as listed on Form OP-SUM (Individual Unit Summary).

SOP/GOP Index No.:

Site operating permit (SOP) applicants should indicate the SOP index number for the unit or group of units (maximum 15 characters consisting of numeric, alphanumeric characters, and/or dashes prefixed by a code for the applicable regulation [i.e., 60IIII-XX]). GOP applicants should indicate the appropriate GOP index number in this column from the applicable GOP table (SSS-FF-XXX). Applicants should complete all applicable GOP attribute information before determining the GOP index number. For additional information relating to SOP index numbers, please go to the TCEQ website at [www.tceq.texas.gov/permitting/air/guidance/titlev/tv\_fop\_guidance.html](https://www.tceq.texas.gov/permitting/air/guidance/titlev/tv_fop_guidance.html).

* Do not complete “Kilowatts” if “Displacement” is “30+.”

Kilowatts:

Select one of the following options to indicate the power rating of the CI ICE expressed in Kilowatts (KW). Enter the code on the form.

For non-emergency and emergency (NOT fire pump) CI ICE manufactured prior to model year 2007

**Code Description**

8- Power rating is less than 8 KW.

8-19 Power rating is greater than or equal to 8 KW and less than 19 KW.

19-37 Power rating is greater than or equal to 19 KW and less than 37 KW.

37-75 Power rating is greater than or equal to 37 KW and less than 75 KW.

75-130 Power rating is greater than or equal to 75 KW and less than 130 KW.

130-2237 Power rating is greater than or equal to 130 KW and less than or equal to 2237 KW.

2237+ Power rating is greater than or equal to 2237 KW.

For non-emergency CI ICE manufactured in model year 2007 and later

For CI ICE with a displacement less than 10 liters per cylinder

**Code Description**

N8- Power rating is less than 8 KW.

N8-19 Power rating is greater than or equal to 8 KW and less than 19 KW.

N19-37 Power rating is greater than or equal to 19 KW and less than 37 KW.

N37-56 Power rating is greater than or equal to 37 KW and less than 56 KW.

N56-75 Power rating is greater than or equal to 56 KW and less than 75 KW.

N75-130 Power rating is greater than or equal to 75 KW and less than 130 KW.

N130-368 Power rating greater than or equal to 130 KW and less than or equal to 368 KW.

N368-560 Power rating is greater than 368 KW and less than 560 KW.

N560-900 Power rating greater than or equal to 560 KW and less than or equal to 900 KW.

N900-2237 Power rating is greater than 900 KW and less than or equal to 2237 KW.

N2237+ Power rating is greater than 2237 KW.

For CI ICE with a displacement greater than or equal to 10 and less than 30 liters per cylinder

**Code Description**

N368-3300 Power rating is greater than 368 KW and less than 3300KW (use only if “Displacement” is

“15-20” and “Model Year” is “2007” through “2013”).

N3300+ Power rating is greater than or equal to 3300 KW (use only if “Displacement” is “15-20” and “Model Year” is “2007” through “2013”).

N75- Power rating is less than 75 KW.

N75-368 Power rating is greater than or equal to 75 KW and less than or equal to 368 KW.

N368-600 Power rating is greater than 368 KW and less than 600 KW.

N600-1400 Power rating is greater than or equal to 600 KW and less than 1400 KW.

N1400-2000 Power rating is greater than or equal to 1400 KW and less than 2000 KW.

N2000-3700 Power rating is greater than or equal to 2000 KW and less than 3700 KW.

N3700+ Power rating is greater than or equal to 3700 KW.

For emergency (NOT fire pump) CI ICE manufactured in model year 2007 and later

For CI ICE with a displacement less than 10 liters per cylinder

**Code Description**

E8- Power rating is less than 8 KW.

E8-19 Power rating is greater than or equal to 8 KW and less than 19 KW.

E19-37 Power rating is greater than or equal to 19 KW and less than 37 KW.

E37-75 Power rating is greater than or equal to 37 KW and less than 75 KW.

E75-130 Power rating is greater than or equal to 75 KW and less than 130 KW.

E130-368 Power rating greater than or equal to 130 KW and less than or equal to 368 KW.

E368-560 Power rating greater than or equal to 368 KW and less than or equal to 560KW.

E560-2237 Power rating is greater than 560 KW and less than or equal to 2237 KW.

E2237+ Power rating is greater than 2237 KW.

For CI ICE with a displacement greater than or equal to 10 and less than 15 liters per cylinder

**Code Description**

E75- Power rating is less than 75 KW.

E75-368 Power rating is greater than or equal to 75 KW and less than or equal to 368 KW.

E368-600 Power rating is greater than 368 KW and less than 600 KW.

E600-1400 Power rating is greater than or equal to 600 KW and less than 1400 KW.

E1400-2000 Power rating is greater than or equal to 1400 KW and less than 2000 KW.

E2000-3700 Power rating is greater than or equal to 2000 KW and less than 3700 KW.

E3700+ Power rating is greater than or equal to 3700 KW.

For CI ICE with a displacement greater than or equal to 15 and less than 20 liters per cylinder

**Code Description**

E368-3300 Power rating is greater than 368 KW and less than 3300 KW (use only if “Model Year” is 2013).

E75- Power rating is less than 75 KW.

E75-368 Power rating is greater than or equal to 75 KW and less than or equal to 368 KW.

E368-600 Power rating is greater than 368 KW and less than 600 KW.

E600-1400 Power rating is greater than or equal to 600 KW and less than 1400 KW.

E1400-2000 Power rating is greater than or equal to 1400 KW and less than 2000 KW.

E2000-3300 Power rating is greater than or equal to 2000 KW and less than 3300 KW.

E3300+ Power rating is greater than or equal to 3300 KW.

For CI ICE with a displacement greater than or equal to 20 and less than 30 liters per cylinder

**Code Description**

E75- Power rating is less than 75 KW.

E75-368 Power rating is greater than or equal to 75 KW and less than or equal to 368 KW.

E368-600 Power rating is greater than 368 KW and less than 600 KW.

E600-1400 Power rating is greater than or equal to 600 KW and less than 1400 KW.

E1400-2000 Power rating is greater than or equal to 1400 KW and less than 2000 KW.

E2000+ Power rating is greater than or equal to 2000 KW.

For ALL fire pump CI ICE less than 30 liters per cylinder

**Code Description**

F8- Power rating is less than 8 KW.

F8-19 Power rating is greater than or equal to 8 KW and less than 19 KW.

F19-37 Power rating is greater than or equal to 19 KW and less than 37 KW.

F37-75 Power rating is greater than or equal to 37 KW and less than 75 KW.

F75-130 Power rating is greater than or equal to 75 KW and less than 130 KW.

F130-368 Power rating is greater than or equal to 130 KW and less than or equal to 368 KW.

F368-450 Power rating is greater than 368 KW and less than 450 KW.

F450-560 Power rating is greater than or equal to 450 KW and less than or equal to 560 KW.

F560+ Power rating is greater than 560 KW.

* Complete “Filter” only if “Service” is “NON.”

Filter:

Enter “YES” if the CI ICE is equipped with a diesel particulate filter. Otherwise, enter “NO.”

* Complete “AECD” only if “Service” is “NON” or “EMERG.”

AECD:

Enter “YES” if the CI ICE is equipped with auxiliary emission control devices (AECDs) pursuant to the requirements of 40 CFR 1039.665. Otherwise, enter “NO”.

* Complete “Standards” only if “Service” is “EMERG” or “FIRE.”

Standards:

Enter “YES” if the emergency CI ICE meets the Tier 1, 2, 3, or 4 standards applicable to non-emergency engines (for the same KW and model year). Otherwise, enter “NO.”

Compliance Option:

Select one of the following options to indicate how compliance is being demonstrated. Enter the code on the form.

Select one of the following two options only if “Commencing” is “MOD” or “RECON.”

**Code Description**

CERT Engine certified to meet the emission standards in §60.4204(e) or §60.4205(f), as applicable.

NONCERT Engine not certified to meet the emission standards in §60.4204(e) or §60.4205(f), as applicable.

Select one of the following five options only if “Commencing” is “CON:” 55Tand

* “Service” is “NON” or “EMERG” and “Displacement” is NOT “30+” and “Model Year” is “2007-”; 55Tor
* “Service” is “FIRE;” 55Tand
* “Kilowatts” is “F8-”, “F8-19”, “F19-37”, or “F37-75” 54T**and54T** “Model Year” is “2010” or prior; or
* “Kilowatts” is “F75-130” 54T**and 54T**“Model Year” is “2009” or prior; or
* “Kilowatts” is “F130-368”, “F368-450”, or “F450-560” 54T**and54T** “Model Year” is “2008” or prior; or
* “Kilowatts” is “F560+” 54T**and54T** “Model Year” is “2007” or prior.

**Code Description**

PURCH Certified engine according to § 60.4211(b)(1).

SIMILAR Records are kept on a similar engine according to § 60.4211(b)(2).

MDATA Records are kept of manufacturer data according to § 60.4211(b)(3).

CDDATA Records are kept of control device data according to § 60.4211(b)(4).

TEST Performance test conducted according to § 60.4211(b)(5).

Select one of the following two options only if “Commencing” is “CON:” 55Tand

* “Service” is “NON” or “EMERG” and “Displacement” is 55Tnot55T “30+” and “Model Year” is 55Tnot55T “2007-”; 55Tor
* “Service” is “FIRE;” 55Tand
* “Kilowatts” is “F8-”, “F8-19”, “F19-37”, or “F37-75” 54T**and54T** “Model Year” is “2011” or later; or
* “Kilowatts” is “F75-130” 54T**and54T** “Model Year” is “2010” or later; or
* “Kilowatts” is “F130-368”, “F368-450”, or “F450-560” 54T**and54T** “Model Year” is “2009” or later; or
* “Kilowatts” is “F560+” 54T**and54T** “Model Year” is “2008” or later.

**Code Description**

MANU YES The CI ICE and control device is installed, configured, operated, and maintained according to the manufacturer’s emission-related written instructions.

MANU NO The CI ICE and control device IS NOT installed, configured, operated, and maintained according to the manufacturer’s emission-related written instructions.

* Complete “PM Compliance” only if “Commencing” is “CON” and “Service” is “NON,” and “Displacement” is “30+.”

PM Compliance:

Select one of the following options to indicate which Particulate Matter compliance option you are using. Enter the code on the form.

**Code Description**

PM60 Particulate matter emissions are reduced by 60% or more

PM15 Particulate matter emissions are limited in the engine exhaust to 0.15 g/KW-hr

* Complete “Options” only if “Service” is “FIRE” and if one of the following conditions are met:
* “Kilowatts” is “F37-75” and “Model Year” is “2011”, “2012,” or “2013”; or
* “Kilowatts” is “F75-130” and “Model Year” is “2010,” “2011”, or “2012”; or
* “Kilowatts” is “F130-368” or “F368-450” and “Model Year” is “2009,” “2010”, or “2011”

Options:

Select one of the following options to indicate the rated speed (in RPMs) and whether or not you are choosing to alternatively comply with the previous model year’s emission limits as stated in 40 CFR 60, Subpart IIII-Table 4 (Footnotes 1-3). Enter the code on the form.

**Code Description**

2650- The CI ICE rated speed is less than 2650 RPMs (Not allowed to comply with the previous model year’s emission limits).

2650+YES The CI ICE rated speed is greater than 2650 RPMs and is complying with the previous model year’s emission limits.

2650+NO The CI ICE rated speed is greater than 2650 RPMs but is not complying with the previous model year’s emission limits.

# Stationary Reciprocating Internal Combustion Engine Attributes

# Form OP-UA2 (Page 1)

# Federal Operating Permit Program

# Table 1a: Title 30 Texas Administrative Code Chapter 117 (30 TAC Chapter 117)

# Subchapter B: Combustion Control at Major Industrial, Commercial, and Institutional Sources in Ozone Nonattainment Areas

# Texas Commission on Environmental Quality

| **Date** | **Permit No.** | **Regulated Entity No.** |
| --- | --- | --- |
|  |  |  |

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Unit ID No.** | **SOP/GOP Index No.** | **Horsepower Rating** | **RACT Date Placed in Service** | **Functionally Identical Replacement** | **Type of Service** | **Fuel Fired** | **Engine Type** | **ESAD Date Placed in Service** | **Diesel HP Rating** |
|  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |

# Stationary Reciprocating Internal Combustion Engine Attributes

# Form OP-UA2 (Page 2)

# Federal Operating Permit Program

# Table 1b: Title 30 Texas Administrative Code Chapter 117 (30 TAC Chapter 117)

# Subchapter B: Combustion Control at Major Industrial, Commercial, and Institutional Sources in Ozone Nonattainment Areas

# Texas Commission on Environmental Quality

| **Date** | **Permit No.** | **Regulated Entity No.** |
| --- | --- | --- |
|  |  |  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Unit ID No.** | **SOP/GOP Index No.** | **NOx Emission Limitation** | **23-C Option** | **30 TAC Chapter 116 Limit** | **EGF System CAP Unit** | **NOx Averaging Method** | **NOx Reduction** | **NOx Monitoring System** |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |

# Stationary Reciprocating Internal Combustion Engine Attributes

# Form OP-UA2 (Page 3)

# Federal Operating Permit Program

# Table 1c: Title 30 Texas Administrative Code Chapter 117 (30 TAC Chapter 117)

# Subchapter B: Combustion Control at Major Industrial, Commercial, and Institutional Sources in Ozone Nonattainment Areas

# Texas Commission on Environmental Quality

| **Date** | **Permit No.** | **Regulated Entity No.** |
| --- | --- | --- |
|  |  |  |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Unit ID No.** | **SOP/GOP Index No.** | **Fuel Flow Monitoring** | **CO Emission Limitation** | **CO Averaging Method** | **CO Monitoring System** | **NH**R**3**R **Emission Limitation** | **NH**R**3**R **Monitoring** |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |

Stationary Reciprocating Internal Combustion Engine Attributes

Form OP-UA2 (Page 4)

Federal Operating Permit Program

Table 2a: Title 40 Code of Federal Regulations Part 63 (40 CFR Part 63)

Subpart ZZZZ: National Emission Standards for Hazardous Air Pollutants for Stationary Reciprocating Internal Combustion Engines

Texas Commission on Environmental Quality

| **Date** | **Permit No.** | **Regulated Entity No.** |
| --- | --- | --- |
|  |  |  |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Unit ID No.** | **SOP/GOP Index No.** | **HAP Source** | **Brake HP** | **Construction/ Reconstruction Date** | **Nonindustrial Emergency Engine** | **Service Type** | **Stationary RICE Type** |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |

Stationary Reciprocating Internal Combustion Engine Attributes

Form OP-UA2 (Page 5)

Federal Operating Permit Program

Table 2b: Title 40 Code of Federal Regulations Part 63 (40 CFR Part 63)

Subpart ZZZZ: National Emission Standards for Hazardous Air Pollutants for Stationary 29BReciprocating Internal Combustion Engines

Texas Commission on Environmental Quality

| **Date** | **Permit No.** | **Regulated Entity No.** |
| --- | --- | --- |
|  |  |  |

| **Unit ID No.** | **SOP/GOP Index No.** | **Manufacture Date** | **Operating Hours** | **Different Schedule** | **Emission Limitation** | **Displacement** |
| --- | --- | --- | --- | --- | --- | --- |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |

Stationary Reciprocating Internal Combustion Engine Attributes

Form OP-UA2 (Page 6)

Federal Operating Permit Program

Table 2c: Title 40 Code of Federal Regulations Part 63 (40 CFR Part 63)

Subpart ZZZZ: National Emission Standards for Hazardous Air Pollutants for Stationary 32BReciprocating Internal Combustion Engines

Texas Commission on Environmental Quality

| **Date** | **Permit No.** | **Regulated Entity No.** |
| --- | --- | --- |
|  |  |  |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Unit ID No.** | **SOP/GOP Index No.** | **Crankcase** | **Performance Test** | **Control Technique** | **Operating Limits** | **Monitoring System** |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |

Stationary Reciprocating Internal Combustion Engine Attributes

Form OP-UA2 (Page 7)

Federal Operating Permit Program

Table 3: Title 30 Texas Administrative Code Chapter 117 (30 TAC Chapter 117) Subchapter E: Multi-Region Combustion Control

Texas Commission on Environmental Quality

| **Date** | **Permit No.** | **Regulated Entity No.** |
| --- | --- | --- |
|  |  |  |

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Unit ID No.** | **SOP/GOP Index No.** | **Unit Type** | **Horsepower Rating** | **Landfill** | **Control Operations** | **NOx and O2 Monitoring** | **Ammonia Use** | **NH**R**3 Emission Limitation** | **Ammonia Monitoring** |
|  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |

Stationary Reciprocating Internal Combustion Engine Attributes

Form OP-UA2 (Page 8)

Federal Operating Permit Program

Table 4a: Title 40 Code of Federal Regulations Part 60 (40 CFR Part 60)

Subpart JJJJ: Standards of Performance for Stationary Spark Ignition Internal Combustion Engines

Texas Commission on Environmental Quality

| **Date** | **Permit No.** | **Regulated Entity No.** |
| --- | --- | --- |
|  |  |  |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Unit ID No.** | **SOP/GOP Index No.** | **Construction/ Reconstruction/ Modification Date** | **Test Cell** | **Exemption** | **Temp Replacement** | **Horsepower** | **Fuel** | **AEL No.** | **Lean Burn** | **Commencing** |
|  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |

Stationary Reciprocating Internal Combustion Engine Attributes

Form OP-UA2 (Page 9)

Federal Operating Permit Program

Table 4b: Title 40 Code of Federal Regulations Part 60 (40 CFR Part 60)

Subpart JJJJ: Standards of Performance for Stationary Spark Ignition Internal Combustion Engines

Texas Commission on Environmental Quality

| **Date** | **Permit No.** | **Regulated Entity No.** |
| --- | --- | --- |
|  |  |  |

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Unit ID No.** | **SOP/GOP Index No.** | **Manufacture Date** | **Displacement** | **Certified** | **Operation** | **Certified Modification** | **Service** | **Severe Duty** | **Optional Compliance** |
|  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |

Stationary Reciprocating Internal Combustion Engine Attributes

Form OP-UA2 (Page 10)

Federal Operating Permit Program

Table 5a: Title 40 Code of Federal Regulations Part 60 (40 CFR Part 60)

Subpart IIII: Standards of Performance for Stationary Compression Ignition Internal Combustion Engines

Texas Commission on Environmental Quality

| **Date** | **Permit No.** | **Regulated Entity No.** |
| --- | --- | --- |
|  |  |  |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Unit ID No.** | **SOP/GOP Index No.** | **54TApplicability Date** | **Exemptions** | **Service** | **Commencing** | **Manufacture Date** |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |

Stationary Reciprocating Internal Combustion Engine Attributes

Form OP-UA2 (Page 11)

Federal Operating Permit Program

Table 5b: Title 40 Code of Federal Regulations Part 60 (40 CFR Part 60)

Subpart IIII: Standards of Performance for Stationary Compression Ignition Internal Combustion Engines

Texas Commission on Environmental Quality

| **Date** | **Permit No.** | **Regulated Entity No.** |
| --- | --- | --- |
|  |  |  |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Unit ID No.** | **SOP/GOP Index No.** | **Diesel** | **AES No.** | **Displacement** | **Generator Set** | **Model Year** | **Install Date** |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |

Stationary Reciprocating Internal Combustion Engine Attributes

Form OP-UA2 (Page 12)

Federal Operating Permit Program

Table 5c: Title 40 Code of Federal Regulations Part 60 (40 CFR Part 60)

Subpart IIII: Standards of Performance for Stationary Compression Ignition Internal Combustion Engines

Texas Commission on Environmental Quality

| **Date** | **Permit No.** | **Regulated Entity No.** |
| --- | --- | --- |
|  |  |  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Unit ID No.** | **SOP/GOP Index No.** | **Kilowatts** | **Filter** | **AECD** | **Standard** | **Compliance Option** | **PM Compliance** | **Options** |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |